ONU Discovered successfully
Testing on ALPHA ONU
BEFORE AUTHENTICATION
=======================================================================
(voltha) devices
Devices:
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
|               id |              type | root |        parent_id | serial_number | admin_state | oper_status | connect_status | parent_port_no |    host_and_port |                               reason | proxy_address.device_id | proxy_address.onu_id | proxy_address.onu_session_id |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
| 00012942badf82b8 |           openolt | True | 000100000a5a0072 |  EC1721000208 |     ENABLED |      ACTIVE |      REACHABLE |                | 10.90.0.114:9191 |                                      |                         |                      |                              |
| 0001deac5dfdfe5e | brcm_openomci_onu |      | 00012942badf82b8 |  ALPHe3d1cfde |     ENABLED |      ACTIVE |      REACHABLE |      536870912 |                  | tech-profile-config-download-success |        00012942badf82b8 |                    1 |                            1 |
| 000160d8d9b90946 | brcm_openomci_onu |      | 00012942badf82b8 |  ISKT71e80080 |    DISABLED |             |      REACHABLE |      536870912 |                  |                      omci-admin-lock |        00012942badf82b8 |                    2 |                            2 |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
(voltha)
=============================================================
# bs /b/e vlan_action
Object: vlan_action/dir=us,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 0
              action : {cmd=push_always+remark+tpid_rem,ovid=4091,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 0
              action : {cmd=pop,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=ds,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
#
========================================================================
PERFORMED FIRST TIME AUTHENTICATION :
SUCCESSFUL
===========================================================================

(voltha) devices
Devices:
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+-------------------+-------------------------+----------------------+------------------------------+
|               id |              type | root |        parent_id | serial_number | admin_state | oper_status | connect_status | parent_port_no |    host_and_port |            reason | proxy_address.device_id | proxy_address.onu_id | proxy_address.onu_session_id |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+-------------------+-------------------------+----------------------+------------------------------+
| 00012942badf82b8 |           openolt | True | 000100000a5a0072 |  EC1721000208 |     ENABLED |      ACTIVE |      REACHABLE |                | 10.90.0.114:9191 |                   |                         |                      |                              |
| 0001deac5dfdfe5e | brcm_openomci_onu |      | 00012942badf82b8 |  ALPHe3d1cfde |     ENABLED |      ACTIVE |      REACHABLE |      536870912 |                  | omci-flows-pushed |        00012942badf82b8 |                    1 |                            1 |
| 000160d8d9b90946 | brcm_openomci_onu |      | 00012942badf82b8 |  ISKT71e80080 |    DISABLED |             |      REACHABLE |      536870912 |                  |   omci-admin-lock |        00012942badf82b8 |                    2 |                            2 |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+-------------------+-------------------------+----------------------+------------------------------+
(voltha)
Device 00012942badf82b8 (type: openolt)
Flows (44):
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
| table_id | priority |    cookie |    in_port | vlan_vid | eth_type | ip_proto | udp_src | udp_dst | set_vlan_vid | pop_vlan | push_vlan |     output | goto-table |      write-metadata | meter |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
|        0 |    10000 | ~9acfb5a4 |      65536 |          |     88CC |          |         |         |              |          |           | CONTROLLER |            |                     |       |
|        0 |    10000 | ~060082f1 |      65536 |          |      800 |       17 |      67 |      68 |              |          |           | CONTROLLER |            |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e | CONTROLLER |     4090 |          |          |         |         |              |          |           |         32 |            |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         |              |          |           | CONTROLLER |            | 1151514404601200640 |     1 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        0 |     1000 | ~951d9d66 |      65536 |      111 |          |          |         |         |              |      Yes |           |            |          1 |   31525472269500432 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        1 |     1000 | ~86a10755 |         16 |      112 |          |          |         |         |          111 |          |      8100 |      65536 |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~7d7a0509 |         16 |          |      800 |       17 |      68 |      67 |              |          |           | CONTROLLER |            |        274877906944 |     2 |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
|        0 |    10000 | ~a4d91d68 | CONTROLLER |     4090 |          |          |         |         |              |          |           |         16 |            |                     |       |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
|        0 |    10000 | ~a4d91d68 |         16 |      112 |     888E |          |         |         |              |          |           | CONTROLLER |            |   31525472269500416 |     2 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+--------------+----------+-----------+------------+------------+---------------------+-------+
(device 00012942badf82b8)

===========================================================================
# bs /b/e vlan_action
Object: vlan_action/dir=us,index=2. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 2
              action : {cmd=replace+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=us,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 1
              action : {cmd=push_always+remark+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 1
              action : {cmd=replace,ovid=0,opbit=0,otpid=0xffff,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 0
              action : {cmd=push_always+remark+tpid_rem,ovid=4091,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 0
              action : {cmd=pop,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=ds,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
#
========================================================================
deviceId=of:000000000a5a0072, flowRuleCount=11
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:67, UDP_DST:68], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:eapol, VLAN_VID:112], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:2, metadata=METADATA:70004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:68, UDP_DST:67], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:2, metadata=METADATA:4000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:546, UDP_DST:547], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:32, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:1, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:547, UDP_DST:546], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:2, metadata=METADATA:4000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:lldp], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=1000, selector=[IN_PORT:65536, VLAN_VID:111], treatment=[immediate=[VLAN_POP], transition=TABLE:1, meter=METER:2, metadata=METADATA:70004000000010/0]
    ADDED, bytes=0, packets=0, table=0, priority=1000, selector=[IN_PORT:16, VLAN_VID:0], treatment=[immediate=[VLAN_ID:112], transition=TABLE:1, meter=METER:2, metadata=METADATA:6f004000010000/0]
    ADDED, bytes=0, packets=0, table=1, priority=1000, selector=[IN_PORT:16, VLAN_VID:112], treatment=[immediate=[VLAN_PUSH:vlan, VLAN_ID:111, OUTPUT:65536], meter=METER:2, metadata=METADATA:4000000000/0]
    ADDED, bytes=0, packets=0, table=1, priority=1000, selector=[IN_PORT:65536, VLAN_VID:112], treatment=[immediate=[VLAN_POP, VLAN_ID:0, OUTPUT:16], meter=METER:2, metadata=METADATA:4000000000/0]
onos>
========================================================================
DISABLED ONU
++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
voltha) devices
Devices:
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+-----------------+-------------------------+----------------------+------------------------------+
|               id |              type | root |        parent_id | serial_number | admin_state | oper_status | connect_status | parent_port_no |    host_and_port |          reason | proxy_address.device_id | proxy_address.onu_id | proxy_address.onu_session_id |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+-----------------+-------------------------+----------------------+------------------------------+
| 00012942badf82b8 |           openolt | True | 000100000a5a0072 |  EC1721000208 |     ENABLED |      ACTIVE |      REACHABLE |                | 10.90.0.114:9191 |                 |                         |                      |                              |
| 0001deac5dfdfe5e | brcm_openomci_onu |      | 00012942badf82b8 |  ALPHe3d1cfde |    DISABLED |             |      REACHABLE |      536870912 |                  | omci-admin-lock |        00012942badf82b8 |                    1 |                            1 |
| 000160d8d9b90946 | brcm_openomci_onu |      | 00012942badf82b8 |  ISKT71e80080 |    DISABLED |             |      REACHABLE |      536870912 |                  | omci-admin-lock |        00012942badf82b8 |                    2 |                            2 |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+-----------------+-------------------------+----------------------+------------------------------+
(voltha)

Device 00012942badf82b8 (type: openolt)
Flows (12):
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
| table_id | priority |    cookie |    in_port | vlan_vid | eth_type | ip_proto | udp_src | udp_dst |     output |      write-metadata | meter |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~9acfb5a4 |      65536 |          |     88CC |          |         |         | CONTROLLER |                     |       |
|        0 |    10000 | ~060082f1 |      65536 |          |      800 |       17 |      67 |      68 | CONTROLLER |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e | CONTROLLER |     4090 |          |          |         |         |         32 |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~20cf059f |         16 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     2 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
(device 00012942badf82b8)
=================================================================================

deviceId=of:000000000a5a0072, flowRuleCount=5
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:67, UDP_DST:68], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:2, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:546, UDP_DST:547], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:32, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:1, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:lldp], treatment=[immediate=[OUTPUT:CONTROLLER]]
onos>
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
Admin Enabled the ONU AGAIN
=========================
(voltha) devices
Devices:
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
|               id |              type | root |        parent_id | serial_number | admin_state | oper_status | connect_status | parent_port_no |    host_and_port |                               reason | proxy_address.device_id | proxy_address.onu_id | proxy_address.onu_session_id |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
| 00012942badf82b8 |           openolt | True | 000100000a5a0072 |  EC1721000208 |     ENABLED |      ACTIVE |      REACHABLE |                | 10.90.0.114:9191 |                                      |                         |                      |                              |
| 0001deac5dfdfe5e | brcm_openomci_onu |      | 00012942badf82b8 |  ALPHe3d1cfde |     ENABLED |      ACTIVE |      REACHABLE |      536870912 |                  | tech-profile-config-download-success |        00012942badf82b8 |                    1 |                            1 |
| 000160d8d9b90946 | brcm_openomci_onu |      | 00012942badf82b8 |  ISKT71e80080 |    DISABLED |             |      REACHABLE |      536870912 |                  |                      omci-admin-lock |        00012942badf82b8 |                    2 |                            2 |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
(voltha)
(device 00012942badf82b8) flows
Device 00012942badf82b8 (type: openolt)
Flows (12):
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
| table_id | priority |    cookie |    in_port | vlan_vid | eth_type | ip_proto | udp_src | udp_dst |     output |      write-metadata | meter |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~9acfb5a4 |      65536 |          |     88CC |          |         |         | CONTROLLER |                     |       |
|        0 |    10000 | ~060082f1 |      65536 |          |      800 |       17 |      67 |      68 | CONTROLLER |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e | CONTROLLER |     4090 |          |          |         |         |         32 |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~20cf059f |         16 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     2 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
(device 00012942bad
==================================================
deviceId=of:000000000a5a0072, flowRuleCount=5
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:67, UDP_DST:68], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:2, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:546, UDP_DST:547], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:32, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:1, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:lldp], treatment=[immediate=[OUTPUT:CONTROLLER]]
onos>
===================================================
# bs /b/e vlan_action
Object: vlan_action/dir=us,index=2. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 2
              action : {cmd=replace+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=us,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 1
              action : {cmd=push_always+remark+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 1
              action : {cmd=replace,ovid=0,opbit=0,otpid=0xffff,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 0
              action : {cmd=push_always+remark+tpid_rem,ovid=4091,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 0
              action : {cmd=pop,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=ds,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
#
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
ONU came up fine as ADMIN ENABLED, AUTHENTICATE ONU SECOND TIME 
AUTH WAS SUCCESSFUL
+++++++++++++++++++++++++++++
(device 00012942badf82b8) exit
(voltha) devices
Devices:
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
|               id |              type | root |        parent_id | serial_number | admin_state | oper_status | connect_status | parent_port_no |    host_and_port |                               reason | proxy_address.device_id | proxy_address.onu_id | proxy_address.onu_session_id |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
| 00012942badf82b8 |           openolt | True | 000100000a5a0072 |  EC1721000208 |     ENABLED |      ACTIVE |      REACHABLE |                | 10.90.0.114:9191 |                                      |                         |                      |                              |
| 0001deac5dfdfe5e | brcm_openomci_onu |      | 00012942badf82b8 |  ALPHe3d1cfde |     ENABLED |      ACTIVE |      REACHABLE |      536870912 |                  | tech-profile-config-download-success |        00012942badf82b8 |                    1 |                            1 |
| 000160d8d9b90946 | brcm_openomci_onu |      | 00012942badf82b8 |  ISKT71e80080 |    DISABLED |             |      REACHABLE |      536870912 |                  |                      omci-admin-lock |        00012942badf82b8 |                    2 |                            2 |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
(voltha)
============================

(device 00012942badf82b8) flows
Device 00012942badf82b8 (type: openolt)
Flows (11):
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
| table_id | priority |    cookie |    in_port | vlan_vid | eth_type | ip_proto | udp_src | udp_dst |     output |      write-metadata | meter |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~9acfb5a4 |      65536 |          |     88CC |          |         |         | CONTROLLER |                     |       |
|        0 |    10000 | ~060082f1 |      65536 |          |      800 |       17 |      67 |      68 | CONTROLLER |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e | CONTROLLER |     4090 |          |          |         |         |         32 |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
(device 00012942badf82b8)

—————————————————————————
# bs /b/e vlan_action
Object: vlan_action/dir=us,index=2. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 2
              action : {cmd=replace+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=us,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 1
              action : {cmd=push_always+remark+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 1
              action : {cmd=replace,ovid=0,opbit=0,otpid=0xffff,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 0
              action : {cmd=push_always+remark+tpid_rem,ovid=4091,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 0
              action : {cmd=pop,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=ds,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
#
—————————————————————————————————

deviceId=of:000000000a5a0072, flowRuleCount=11
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:67, UDP_DST:68], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:eapol, VLAN_VID:112], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:3, metadata=METADATA:70004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:68, UDP_DST:67], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:3, metadata=METADATA:4000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:546, UDP_DST:547], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:32, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:1, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:547, UDP_DST:546], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:3, metadata=METADATA:4000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:lldp], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=1000, selector=[IN_PORT:65536, VLAN_VID:111], treatment=[immediate=[VLAN_POP], transition=TABLE:1, meter=METER:3, metadata=METADATA:70004000000010/0]
    ADDED, bytes=0, packets=0, table=0, priority=1000, selector=[IN_PORT:16, VLAN_VID:0], treatment=[immediate=[VLAN_ID:112], transition=TABLE:1, meter=METER:3, metadata=METADATA:6f004000010000/0]
    ADDED, bytes=0, packets=0, table=1, priority=1000, selector=[IN_PORT:16, VLAN_VID:112], treatment=[immediate=[VLAN_PUSH:vlan, VLAN_ID:111, OUTPUT:65536], meter=METER:3, metadata=METADATA:4000000000/0]
    ADDED, bytes=0, packets=0, table=1, priority=1000, selector=[IN_PORT:65536, VLAN_VID:112], treatment=[immediate=[VLAN_POP, VLAN_ID:0, OUTPUT:16], meter=METER:3, metadata=METADATA:4000000000/0]
onos>
———————————————
++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
ADMIN DISABLED and ENABLED
Performed Auth 3rd time
AUTH FAILED
————————————————————————————————————
(voltha) devices
Devices:
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
|               id |              type | root |        parent_id | serial_number | admin_state | oper_status | connect_status | parent_port_no |    host_and_port |                               reason | proxy_address.device_id | proxy_address.onu_id | proxy_address.onu_session_id |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
| 00012942badf82b8 |           openolt | True | 000100000a5a0072 |  EC1721000208 |     ENABLED |      ACTIVE |      REACHABLE |                | 10.90.0.114:9191 |                                      |                         |                      |                              |
| 0001deac5dfdfe5e | brcm_openomci_onu |      | 00012942badf82b8 |  ALPHe3d1cfde |     ENABLED |      ACTIVE |      REACHABLE |      536870912 |                  | tech-profile-config-download-success |        00012942badf82b8 |                    1 |                            1 |
| 000160d8d9b90946 | brcm_openomci_onu |      | 00012942badf82b8 |  ISKT71e80080 |    DISABLED |             |      REACHABLE |      536870912 |                  |                      omci-admin-lock |        00012942badf82b8 |                    2 |                            2 |
+------------------+-------------------+------+------------------+---------------+-------------+-------------+----------------+----------------+------------------+--------------------------------------+-------------------------+----------------------+------------------------------+
(voltha)

(device 00012942badf82b8) flows
Device 00012942badf82b8 (type: openolt)
Flows (11):
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
| table_id | priority |    cookie |    in_port | vlan_vid | eth_type | ip_proto | udp_src | udp_dst |     output |      write-metadata | meter |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~9acfb5a4 |      65536 |          |     88CC |          |         |         | CONTROLLER |                     |       |
|        0 |    10000 | ~060082f1 |      65536 |          |      800 |       17 |      67 |      68 | CONTROLLER |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e | CONTROLLER |     4090 |          |          |         |         |         32 |                     |       |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
|        0 |    10000 | ~f63b131e |         32 |     4091 |     888E |          |         |         | CONTROLLER | 1151514404601200640 |     1 |
+----------+----------+-----------+------------+----------+----------+----------+---------+---------+------------+---------------------+-------+
(device 00012942badf82b8)
==================================================
deviceId=of:000000000a5a0072, flowRuleCount=5
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv4, IP_PROTO:17, UDP_SRC:67, UDP_DST:68], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:16, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:2, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:ipv6, IP_PROTO:17, UDP_SRC:546, UDP_DST:547], treatment=[immediate=[OUTPUT:CONTROLLER]]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:32, ETH_TYPE:eapol, VLAN_VID:4091], treatment=[immediate=[OUTPUT:CONTROLLER], meter=METER:1, metadata=METADATA:ffb004000000000/0]
    ADDED, bytes=0, packets=0, table=0, priority=10000, selector=[IN_PORT:65536, ETH_TYPE:lldp], treatment=[immediate=[OUTPUT:CONTROLLER]]
onos>
====================================
# bs /b/e vlan_action
Object: vlan_action/dir=us,index=2. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 2
              action : {cmd=replace+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=us,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 1
              action : {cmd=push_always+remark+tpid_rem,ovid=112,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=1. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 1
              action : {cmd=replace,ovid=0,opbit=0,otpid=0xffff,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 0
              action : {cmd=push_always+remark+tpid_rem,ovid=4091,opbit=0,otpid=0x8100,ivid=0,ipbit=0,itpid=0xffff}
Object: vlan_action/dir=ds,index=0. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 0
              action : {cmd=pop,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=us,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : us
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
Object: vlan_action/dir=ds,index=127. Object type: vlan_action. Owned by: system
==============================
                 dir : ds
               index : 127
              action : {cmd=0,ovid=0,opbit=0,otpid=0x0,ivid=0,ipbit=0,itpid=0x0}
#
—————————————————————————————————————————————
AUTH failed 4th time as well, errors from voltha 
————————————————————————————————————
20190522T211809.871 ERROR    MainThread brcm_openomci_onu_handler._execute_queued_tp_task {'vcore_id': '0001', 'uni_id': 0, 'instance_id': 'vcore-0_1558477973', 'error': AttributeError("'str' object has no attribute 'clear'",), 'event': 'tech-profile-congiuration-failed', 'device_id': '0001deac5dfdfe5e'}
20190522T211811.109 ERROR    MainThread openolt_flow_mgr.update_logical_flows {'e': AssertionError(), 'ip': '10.90.0.114:9191', 'flow': priority: 10000
20190522T211811.123 ERROR    MainThread openolt_flow_mgr.repush_all_different_flows {'exception': 'Traceback (most recent call last):\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 1099, in repush_all_different_flows\n    self.add_flow(logical_flow)\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 296, in add_flow\n    classifier_info, action_info, flow, tp_id, us_meter_id, ds_meter_id)\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 424, in divide_and_add_flow\n    self.create_us_scheduler_queues(intf_id, onu_id, uni_id, tp_instance, us_meter_id)\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 618, in create_us_scheduler_queues\n    assert kv_store_meter_id == us_meter_id\nAssertionError', 'e': AssertionError(), 'ip': '10.90.0.114:9191', 'instance_id': 'vcore-0_1558477973', 'vcore_id': '0001', 'event': 'Problem reading this flow'}
20190522T212555.196 ERROR    MainThread brcm_openomci_onu_handler._execute_queued_tp_task {'vcore_id': '0001', 'uni_id': 0, 'instance_id': 'vcore-0_1558477973', 'error': AttributeError("'str' object has no attribute 'clear'",), 'event': 'tech-profile-congiuration-failed', 'device_id': '0001deac5dfdfe5e'}
20190522T212555.307 ERROR    MainThread openolt_flow_mgr.update_logical_flows {'e': AssertionError(), 'ip': '10.90.0.114:9191', 'flow': priority: 10000
20190522T212555.320 ERROR    MainThread openolt_flow_mgr.repush_all_different_flows {'exception': 'Traceback (most recent call last):\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 1099, in repush_all_different_flows\n    self.add_flow(logical_flow)\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 296, in add_flow\n    classifier_info, action_info, flow, tp_id, us_meter_id, ds_meter_id)\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 424, in divide_and_add_flow\n    self.create_us_scheduler_queues(intf_id, onu_id, uni_id, tp_instance, us_meter_id)\n  File "/voltha/voltha/adapters/openolt/openolt_flow_mgr.py", line 618, in create_us_scheduler_queues\n    assert kv_store_meter_id == us_meter_id\nAssertionError', 'e': AssertionError(), 'ip': '10.90.0.114:9191', 'instance_id': 'vcore-0_1558477973', 'vcore_id': '0001', 'event': 'Problem reading this flow'}